Red +12V
Black GND
White CAN H
Green CAN L
Yellow K-Line
Blue-green GPT1 Scanmatik OR GPT0 GREY KTM bench pinout
Yellow-red GPT2 Scanmatik OR GPT1BLUE KTM bench pinout
Purple Vpp
Blue-CNF1
Grey boot
External power supply 12 V (5 A max) Jack



The feature of the first party: the wires CAN white and green swapped! Ping before connecting. Correct Pinout DB25-8 - white - CAN-H. DB25-9 - green - CAN-L

Pinout:
Red +12V
Black GND
White CAN H
Green CAN L
Yellow K-Line
Blue-green GPT1
Yellow-red GPT2
Purple Vpp
Blue-CNF1
Grey boot
External power supply 12 V (5 A max) Jack
Led - power on BU included
Power management and auto signals is performed by the program PCMFlash.

My peugeot cable 
purple white can lo
pink white can hi
turquioe +12
blue white +12
